Quality Clause 240304 - CMM Dimensional Inspection (07/01/2025 - Rev A)

Actual dimensions and locations toleranced to three (3) decimal places shall be

measured and recorded using a calibrated coordinate measurement machine (CMM). All

other dimensions can be measured with conventional hand-measuring tools. All actual

dimensional readings shall be provided.